Create provider, init position

For consumer in consumer\_list:

Cacluate provider to consumer trajectory first x then y

If trajectory change direction:

If transmiter not exist:

Create transmiter

Transmiter input/output stream setting

Provider output stream setting

Else:

Transimiter output stream setting

Else:

Provider output stream setting